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Context and Business Requirements 
	This section provides the context to this Modification Proposal and summarises the key business requirements for it, as currently clarified and refined by the Working Group. 


Context:
Currently, there is no standardised way of describing ALCS and HCALCS. When adding a switch description to the ESME, the only constraint is the length of the description – it must not be more than 127 characters long. Each supplier could have its own nomenclature for naming ALCS and HCALCS, for example it may or may not reflect what is connected to a switch. There is also a risk that the nomenclature may not be transparent enough to a supplier which gained the Smart Metering System following a CoS event. The lack of understanding of what is connected to each switch, may lead the new supplier to apply the wrong settings to an ALCS and adversely impact the customer.  
SECMP0019 suggests introducing a standardised nomenclature for ALCS and HCALCS such that the description of what is connected to the switch becomes transparent. 
Proposed Governance Arrangements:   
SECMP0019 would develop an ALCS/HCALCS Labels Requirements Document. This document would set out:
a) The content of the list – i.e. the information required to describe in detail what may be connected to the switch, 
b) The naming convention for the associated label; 
c) Any validation for the label field (for example, that the label is no longer than 22 characters); and 
d) How new labels will be added to the list (i.e. what are the conditions of a valid entry.) 
This document would become part of the SEC. 
Question: to discuss at next Working Group  
It is then proposed that on behalf of the Panel, the TABASC, would be responsible for establishing and maintaining a list of ALCS/HCALCS labels and their associated descriptions (the “ALCS/HCALCS Labels List”). 
[Parties] wishing to add a label to the ALCS/HCALCS Labels List would make a valid submission as set in the ALCS/HCALCS Labels Requirements Document to the Panel. SECAS will be managing this process on behalf of the Panel. The Panel (the TABASC on the Panel’s behalf) would assess the submission and if the submission is valid, update the ALCS/HCALCS Labels List. 
Question: who should be eligible to request that a label is added to the ALCS/HCALCS Labels List? Any Party or just Import Suppliers?
Business Requirements:
Notify the Parties that the list has been updated
1. The ALCS/HCALCS Labels List will be sent to DCC when the list is updated. As part of the Impact Assessment, the DCC is asked to confirm how the DCC would like to receive the file and the format of it.  
2. The DCC will be allowed 24 hours from the receipt of the list to make any modifications to its systems to reflect the updated list. 
3. When the DCC receives SRV 6.14.1, the DCC will ensure that the “SwitchDescription” in SRV 6.14.1 matches an entry on the ALCS/HCALCS List stored in the DCC System. 
Any SRV 6.14.1 that contains a “SwitchDescription” that is not on the ALCS/HCALCS list will be rejected by the DCC.

Legal Instructions 
	This section details the required changes to the regulatory framework that are proposed to implement the requirements for this Modification Proposal. Where changes to the regulatory framework are made, they are highlighted in red text. For clarity, deletion is shown by strike through and addition is shown by underlining. 



SEC Appendix AD - DCC User Interface Specification 
ALCSHCALCSDescription Definition
	Data Item
	Description / Valid Set 
	Type
	Mandatory
	Default
	Units

	SwitchDescription
	The description of the ALC or HCALC Switch
Valid set:
· All printable characters, i.e. characters with ASCII values of 32 (space) to 126 (tilde) inclusive
· SwitchDescription shall match an entry in the ALCS/HCALS List.  
	Restriction of xs:string (maxLength = 127,
pattern = “[ -~]+”)

	Yes
	None
	N/A

	Index

(attribute of ALCSHCALCSDescription)

	The ID of the ALCS/HCALCS
Numerically ordered, not necessarily consecutive.
	sr:range_1_5

(xs:positiveInteger minInclusive 1 maxInclusive 5)
	Yes
	None
	N/A


Table 172 : ALCSHCALCSDescription (sr:ALCSHCALCSDescription) data items
SEC Section F – Smart Metering System Requirements
F5	ALCS/HCALCS Labels List
F5.1	The Panel will establish and maintain an ALCS/HCALCS Labels List.  The Panel will ensure that the ALCS/HCALCS Labels List is populated and updated in accordance with the ALCS/HCALCS Requirements Document. 
F5.2	Within one working day after the ALCS/HCALCS Labels List is updated, the Panel will:
a) Provide the updated content to the DCC;
b) Publish a copy of the updated list on the website; and 
c) Notify the Parties that the list has been updated. 
F5.3	Within 24 hours from receiving the updated content the DCC will make any necessary updates to its systems to reflect the changes to the list. 

Appendix [tbc] – ALCS/HCALCS Labels Requirements Document
[tbc – for discussion at next Working Group] 

Appendix – Acronyms 
	Acronym 

	Definition 

	ALCS
	Auxiliary Load Control Switch

	CoS
	Change of Supplier 

	DCC
	Data and Communications Company

	HCALCS
	HAN Controlled Auxiliary Load Control Switch
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